

FOR IMMEDIATE RELEASE

  **BMR Suspension Lowering Springs 2" Drop for 1978- 1987 G-Body**

**SP463 - $269.95**

Improve the cosmetic appeal and increase the handling capabilities of your 1978-1987 G-Body with Lowering Springs from BMR Suspension. Manufactured from chrome silicon high-tensile spring wire, these springs are cold wound on a CNC coiling machine that can adjust the spring diameter in real time to ensure that every spring is exactly the same. These springs will lower your 1978-1987 G-Body 2” in the front and rear. They feature a linear working spring rate to give you a smooth ride and great looks. BMR Lowering Springs (SP463) will lower the center of gravity and increase the cornering capabilities of your G-Body without sacrificing ride quality. BMR designed the SP463 springs for street performance, but will also work well for the occasional track outing. Like all BMR lowering springs, the SP463 has a LIFETIME guarantee against spring sag. Front springs (SP464) and rear springs (SP465) are also sold separately. Available in red powdercoat for long-lasting good looks. Installation time is about 2-3 hours. Proudly built in America with American steel!

To preview all of BMR’s high-performance suspension parts, please visit [www.bmrsuspension.com,](http://www.bmrsuspension.com/) email sales@bmrsuspension.com, or contact them at BMR Suspension, 928 Sligh Ave, Seffner, FL 33584, 813-986-9302, Fax: 813-986-8055.

Editors: *Download this press release and high resolution images at*[*: www.bmrsuspension.com/?page=pressrelease*](file://Volumes/BMR%20Server%20Shared/Press%20Releases/www.bmrsuspension.com/%253fpage%3Dpressrelease)