

FOR IMMEDIATE RELEASE

**BMR K-Member, Low Mount Turbo, LS1 Motor Mounts, Std Rack Mounts for 93-02 F-Body**

**KM344 - $619.95**

Decrease front end weight and provide extra clearance for low mount turbos in your 1993-2002 F-Body with a K-Member from BMR Suspension. The K-Member is constructed from DOM steel tubing and 3/16” laser-cut mounting plates for uncompromised strength and durability. The BMR Low Mount Turbo K-Member (KM344) has high-clearance vertical motor stands that provide an unobstructed direct air inlet routing to the compressors when running twin low mount turbochargers. The motor stands utilize low-profile, high-density polyurethane bushings relocated down low, away from the heat of the turbochargers. Additionally, this version of the K-member has revised tube positions to provide the most clearance possible around the turbos. This BMR K-Member is both stronger and lighter than the factory stamped steel design. Installation time is 4-6 hours. Available in black hammertone or red powdercoat.

To preview all of BMR’s high-performance suspension parts, please visit [www.bmrsuspension.com](http://www.bmrsuspension.com), email [sales@bmrsuspension.com](mailto:sales@bmrsuspension.com), or contact them at BMR Suspension, 928 Sligh Avenue, Seffner, FL 33584, 813-986-9302, Fax: 813-986-8055.